**M.7.2. Terminal Capabilities – 9F33**

**Byte 1**

bit 8: 1 = Manual Key Entry

bit 7: 1 = Magnetic Stripe

bit 6: 1 = IC with contacts

bit 5: 1 = RFU

bit 4: 1 = RFU

bit 3: 1 = RFU

bit 2: 1 = RFU

bit 1: 1 = RFU

**Byte 2**

bit 8: 1 = Plaintext PIN for ICC verification

bit 7: 1 = Enciphered PIN for online verification

bit 6: 1 = Signature (paper)

bit 5: 1 = Enciphered PIN for offline verification

bit 4: 1 = No CVM Required

bit 3: = RFU

bit 2: = RFU

bit 1: = RFU

**Byte 3**

bit 8: 1 = SDA

bit 7: 1 = DDA

bit 6: 1 = Card capture

bit 5: 1 = RFU

bit 4: 1 = CDA

bit 3: = RFU

bit 2: = RFU

bit 1: = RFU

ACUTAL: 60 D0 C8

PROPOSED: 60 F0 C8