**Switching Between SRED key Slot 0 and Slot 8**

**Switch device from slot 0 and slot 8**

1. Make sure slot 8 key is loaded on the device  
 Supervisor > Security > Key status > ADE

2. Load the dl.bundle.Sphere\_config20191210b8.tar MxDownloader, find the file from below path:

T:\Department Private Folders\Business Development\Business Administration\Payment App\5\_TC IPA\IPA5\Verifone\VIPA\Verifone\_Sample\_Config\2020-01-22

3. Reboot the device

4. Now the device is on slot 8

**Switch device from slot 8 to slot 0**

1. Load the dl.bundle.Sphere\_config2.tar

2. Reboot device

3. Now the device is using slot 0

\*After configured to the desired slot to be used on the device, make sure to register the BDK on the CDB for the custID

**BDK** (Base Derivation Key): 0123456789ABCDEFFEDCBA9876543210

